NEW FEATURES:

UPDATES:
•	Future Updates (see the main menu) to Delair can be downloaded from the Internet.

NEW OEM PRODUCTS:	
•	New Models G18-13 and G18-13-2 have been added to the G and G-2 Series.
•	New Models 918-13 and 918-13-2 have been added to the 900 and 900-2 Series.

DPL WIZARD:
•	The new DPL Wizard automates the enclosure and outlet performance correction factors.

UPDATES:
•	Future Updates (see the main menu) to Delair can be downloaded from the Internet.

DELCAD:
•	Drawings for all products are now available in the .dwg format.							
200/9200 SERIES OPTIONS:
•	Dimensional drawings are now available for viewing on screen or printout, for Filter Sections, Filtered Intake Hoods, HC Coils, and CWC Coils.

UTILITIES:

DELHI PULLEY CROSS-REFERENCE 
•	A cross-reference of Browning, Maska, and Woods pulleys is provided in a .pdf format for on screen viewing or printing.

FAN LAWS
•	The Fan Law calculations can now be printed.

DRIVES SELECTION:

PULLEY MANUFACTURER DESIGNATION
•	When making a Drive Selection the user can select Browning, Maska or Woods model designations to appear on the drive list printout and submittal.	

MINIMUM MOTOR HP
•	For the BI and CMRE Series the program will now automatically select the minimum recommended HP (as shown in the catalogue) to handle the startup torque. For example if a BI-13 is selected for 1500 CFM at 0.50" SP, it requires only 0.27 BHP, so a 1/3 HP motor is sufficient. However, the program will select a 1/2 HP motor.

SUBMITTAL:

SOUND POWER LEVEL STATEMENT
•	The submittal now contains the statement, "Sound Power Level @ Frequency, re: 10^12 watts" as it appears on screen. Previously this statement did not appear on the submittal.

NON-CERTIFIED (AMCA) PRODUCTS
•	The submittal performance curve now contains a statement that the air performance data was obtained in a laboratory accredited by AMCA.

REVISIONS:

PRINT LIST
•	The Print List will now print all blowers shown for a selection, or the user can select how many are to be printed. Previously only the top ten would be printed. The Print List also, now shows the dBA sound values on the printout.

AIR AND SOUND PERFORMANCE DATA
•	Performance data has been updated for various models as per recent AMCA check tests such as, Model 307, Model 927, a Model 927-2.

AIR PERFORMANCE DATA
•	Models G15, 815, 915, etc., have had performance improvements.

DRIVE SELECTION PROGRAM
•	When going directly into the Drive Selection program the 200, 200-2, 9200, 9200-2, 9200VIB, 9200VIB2, 300, 600, 700, SIS, BI, CMRE, and DPL now defaults to the standard "Motor Position" when doing a selection. Previously, if the motor position was not selected, the wrong center distance was shown, resulting in an incorrect belt length. 
•	The light duty 1VL, 8325, MVL, AK, AL, MA, and MFAL pulleys that were limited to 3/4 HP are now rated and selected up to 2 HP applications.
•	Model 9218-2 selection of drives for a 213T/215T, 10 HP motor is now available. Previously, a selection for 182T/184T, 7-1/2HP was the maximum.
•	Model 915-10 maximum HP has been revised from 20 HP to the correct value of 10 HP. 
•	Model 915 maximum HP has been revised from 20 HP to the correct value of 15 HP.
•	The program would not select drives for BIDI-16 to 27, and DPL-30 to 36 selections under 5 HP because   1-11/16", 1-15/16" and 2-1/4" bushings are not available for single groove (single groove pulleys are selected up to 5 HP) pulleys. The program now selects two groove pulleys for these Models.
•	The screen display and printout will now show all the characters for the "5VX1000, etc." belts. Previously only "5VX100, etc. was displayed.

REPORTS	
•	The function has been corrected, for the feature of being able to e-mail submittals directly from the submittal preview screen.

DISCHARGE ROTATION SCREEN 600 & BI
•	The 600 and BI discharge rotation selection screen now references units as "Standard" instead of "Stock". 

COMPONENT INFORMATION
•	The reference to "Maximum Bearing RPM" has been deleted to be consistent with the O.E.M.            Catalogue. 

DRAWINGS
•	The BIDI Series "C" shaft to frame location dimension has been added to the drawing.
•	The 9200-2, and 9200-VIB2 drawing has been revised to clarify the cabinet twinning, and from showing two "A" dimensions to show an "A2" dimension which is consistent with the catalogue.
•	The SIS Series drawing has the "M" dimension added as per the catalogue.
•	 The BI-30, 33 & 36-height dimension "A" has been corrected (catalogue to be corrected).

OTHER	
•	The VIB and VIB-2 models have been deleted as a separate Series. The 9200 Series models with internal vibration isolators (VIB) can now be selected under the 9200 Series "Options".
•	The Model 9212VIB2 part number has been revised from 9020312 to the correct number 9020313. 
•	The HC-15 "A" dimension has been corrected (no change to the product) to 32-1/2".
•	The Graphics Server has been updated to Version 6.0. This will eliminate the possibility of the program being disabled if software with newer versions is installed. This was evident if the message; "You do not have an appropriate license to use this functionality." appeared.
•	The shaft and bearing size on Models 920, 922 and 925 single and twins and Model 9220-2 has been revised from 2-1/4” to 2-3/16”